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Stationary Asphalt Plant
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 Double-drum Mobile Asphalt Plant
[bookmark: _GoBack][image: 1717550121042]
image1.jpeg




image2.png
TR AR PERE gﬂ(Technical per[onnance and paramters)
T T T T T T

4EPefE7) Capacity 15th
SR i Diesel 41.5kw 54kw 635kw 1045 kw, 125k
Total Power i Coal 57.5kw 75kw 865 kw 1275 kw 169 kw
EEE1E AG Batcher 3m'x3 3mx3 3mx3 Smix3 5mix3
FEE Asphalt storage hopper 3t 5t 5t 9t 9t
T 20 ™ 100 10 0
REGE ($/5%)

barrel rotation speed (rotation/min) 18 8 16 16 16

JERIEE sphere of application iH&E®. H&EWA. HEREMRL  asphalt powder, asphalt aggregate, asphalt concrete

AR Product Temp 120-1802T 8 F5
WRRIEHE Fuel consumption RO 5-7.5kg/, HAfCoal:13-15kg/t
7= Production cycle 3940 EMSIS204R% 3 minutes, i.e. 20 batches per hour

&iE L EARMGERE , Qftes  HTLRESFERHTREERES
Note: Above e standard configurationfor eference). We can moy according to your requiremens.
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i%&ﬁﬁfﬁﬁ;&(Technical performance and paramters)

Eyi ) Capamy 96th 120th 160th 240th
BHREREN Micer 600kg 1000kg 1200kg 1500kg 2000kg 3000kg
#R-E A Hot bin capacity 10m® 15m® 15m? 25m® 40m* 50m*

BEAG +05% +05% *05% +05% +05% £0.5%
1BE 5 %

b 03% =0.3% +03% 03% *03% 03%

Accuracy % Bitumen

B3} Filler =0.3% =0.3% +03% =03% +03% +03%
/I Total power 150kw. 195kw. 220kw. 285kw. 365kw 450kw
FREFEREE Product Temp 120-180 Celsius

WAEHEFE Fuel cons imption 6.5kg/t

#iE : U EARMIRERE | (MeF  talREEFEXHTRERRAES
Note: Above are standard configurationifor reference). We can modify according to your requirements.
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]‘Eﬁfkﬁﬂiﬁﬁgﬂ(Technical performance and paramters)

E7fE Capacity 10th 15th 2t 30

BHIhE W5 Diesel 23kw 27 kw 32kw 45 kw 63 kw
Total Power iy Coal 9kw a3kw 51w 0kw 84k
K AG Batcher 3xam 3xamt 3xam 3xam® 3x5m?
UGG Asphalt storage hopper 51 st 5t 5t 9t

Bl Product Temp 120-1808] 5 Celsius

WREHHIE Fuel consumption MAHOII: 5-8kg/t, MAIRCoal:13-15kg/t
#7530 Control method FIRIEHIEE/PLC

&t UEARMRERER  Rite% , BAIRBEFBERETREREAS
Note: Above are standard confiqurationio eference). W can maify according to your requirements.





